

VOLT / BID
DEMONSTRATION  /  VB-001
Distribution transformer
33 / 0.4 kV  |  Technical schedule
Supply of oil-immersed distribution transformers for an overseas power project.
01   TECHNICAL REQUIREMENTS
02   SCOPE OF SUPPLY
- Complete units, standard accessories and terminal connections.
- Routine test reports and installation documentation in English.
Delivery requirements and site conditions remain subject to confirmation.
Synthetic sample for product demonstration. Not a live tender.
	Parameter
	Requirement

	Rated power
	500 kVA

	Primary / secondary voltage
	33 / 0.4 kV

	Rated frequency
	50 Hz

	Cooling method
	ONAN

	Installation
	Outdoor

	Supply quantity
	6 units









